**HeartGuide™ Wearable Blood Pressure Monitor (BP800M)**

|  |  |
| --- | --- |
| **HeartGuide**™ is the **first wearable blood pressure monitor** in the compact form of a wrist watch – for those who want to keep watch on their heart health, anywhere and take action for their heart health.   * The sleek and stylish HeartGuide™ uses an **inflatable oscillometric blood pressure cuff** -- the same technology used in a doctor’s office -- to ensure accurate and reliable readings. * **HeartGuide**® **received 510K FDA clearance as a medical device.** * HeartGuide® **accurately measures blood pressure, daily activity (including steps, distance and calories burned), pulse rate and sleep quality**. It also functions as a smartwatch, where users can receive text, call and email notifications. * Omron has filed has **more than 80 new patents** for the innovations and new technologies developed to create HeartGuide® in the compact form of a wrist watch. Some of the pumps and valves in HeartGuide® are no larger than a grain of rice. * HeartGuide® holds up to 100 measurements in memory and connects exclusively with Omron’s new **Heart*Advisor***™ app, which stores and tracks heart health data and provides insights and personalized coaching to help users take action for their heart health. * A typical user can expect to charge HeartGuide approximately 2-3 times per week, depending upon the frequency of use of HeartGuide®’s features. * Currently available in size medium (fitting 75% of individuals); small and large sizes will be available later this year. | |
|  | |
| **Specifications** | Diameter approximately 1.89” (48 mm)  Case thickness approximately 0.55” (14 mm)  Band width approximately 1.18” (30 mm) | |
| **Availability & MSRP** | OmronHealthcare.com; $499 (USD) | |
| **Media Contact** | MWWPR for Omron Healthcare / Katherine Clark / 312.981.8548 / [kclark@mww.com](mailto:kclark@mww.com) | |
| **More Information** | <https://omronhealthcare.com/heartguide-wearable-blood-pressure-monitor-bp8000m/> | |

\**High-res images available upon request*